INPUT:

Number of Electrons

at Sense Wire

Avalanche Gas Gain

HV Settings

Signal Generation

Anode Signal needs

determined by

Saturation

Effects are

imporatant

Ion Production

Electron Production determines

Electron Motion Ion Motion

Collection on

Sense Wire

Collection on

Frisch Grid

Cathode Signal

Pad Plane Geometry

H

Pad Response Function induces

determined by

H Cross-Talk induces

OUTPUT:

V(t) on each

Pad

StTrs:

Charge Collection and Signal Generation

determines

File: C:\TpcResponseSimulator\TpcResponseSimulator.mdl Fri Mar 20 17:22:20 1998 State Diagram: Charge Collection Page 1