Output Clocking Logic

FEE Clocking Logic

DAQ_FOL

CLOCK&TRIG_RDO

Config Info

1

OUTPUT_ TIMING

RDO Slow Controls I’face

Temperature Sensor & Power Cntl

RDO/FEE

Power Regulation

Event Cntr

Scan ADC

DATE:

UPDATED BY:

CREATED BY:

DCV_OUT

1 SC_ON_DETECT

FEE_DATA<0:11>

1 1 TEMPERATURE

1

1

Paul Barale � June 2, 1994

UPDATED:

February 25, 1994

Paul Barale �

FEE_SIGNAL

FEE_SIGNAL

FEE_BIAS

FEE_PWR

18-to-1 MUX Laser Diode

GLINK FiberOptic Control

FEE_DATA <12> --> FEE_ADDR <5> <-- FEE_PWR <10> <-- FEE_BIAS <4> <-- FEE_TIMING <6> <-- FEE_CONTROL <10> <-- SPARE <2>

1 up to 9 inputs per RDO card . . . 1

GEOGRAPHIC_ID [9 BITS]

FEE_1.1.1.1.1.2

FEE_ADDRESS

FEE_TIMING

OUTPUT_ADDRESS

FEE ReadOut Card

Event Mem.

FEE Bias Generation