BASE DE DONNEES :

TRAITEMENT :

MATIERE :

TOLERANCES

GENERALES

RUGOSITE

GENERALE

PROTECTION :

Indice

Date

Modifications

Dess

Ech.QSUBATECH

 IN2P3,EMN

UNIVERSITE

SCRM

Dessine

ECOLE DES MINES  4 rue Alfred Kastler

La Chantrerie 44070 NANTES Cedex 03

  Tel 51 85 81 00 -Fax 51 85 84 79

IndiceSSD,ETUDSTAR

/0NE/TWO LADDERS TO TRY

VIEWS FOR EXPLCATION

G.Guilloux

14/5/02

240EET134

PIECES OF THE CONE TO ATTACH SSD OR ONE LADDER
SHIELDING RINGS

DRAWING Q243DET133

DETACHABLE PIN

TO PUT IN PLACE THE ONE/TWO LADDERS

WITH SAFETY TOWARDS SVT

VIEW THROUGH THE CONE (WITHOUT CONE)

KNEE*
PIECE TO SUPPORT ONE  LADDER

MOUNTING ON THE TWO KNEES

DRAWING Q243DET136

SVT CABLES WAY

SVT WATER BOXES

SVT CABLES WAY

SUPPLEMANTARY PIECE (Q243DET135)FOR AIR FLOW WAY FROM
THE INNER FIELD CAGE NEAR THE AIR TUBE LADDER.

IN THE CENTRAL HOLE THERE IS A CONDUCTIVE AND SCREEN

FOR IN AIR FLOW.

FOR THE SSD BARREL THERE ARE 10 PIECES ON EACH RING.

THE OTHER TUBES,AIR OUT TUBES, ARE CONNECT AT THE TYGON TUBES

TOWARDS THE END OF THE CONE.

THE SHIELDING WILL BE HOLD ON THE SHIELDING RING AND ON

THESE PIECES WITH A CONDUCTIVE AND ADHESIVE TAPE.

KNEE*TOP VIEW AFTER ROTATION OF 45

 AROUND Z

LADDER AXIS

END OF THE CONE

37 (1.456)
44,5 (1.752)

114,70

INTERFACE PIECES BETWEEN CONE AND SHIELDING RINGS

WITH SVT CABLES WAY

DRAWING Q243DET132

* KNEES

TWO KNEES ARE MOUNTING AT EACH EXTREMITY OF THE TWO LADDERS

THE PIECE BEETWEN THE KNEE AND THE LADDER OLD THE LADDERS,

BE MOUNT IN THE KNEES AND CAN PERMIT A TUNNING

ZYX