SVT Electronics Carrier Assembly Labeling

Version Number: 1.0

Date: 24-Aug-99

Input: SVT cone cable labeling scheme - April 99

Definitions:

A.) Layers 1,3,5 are long ladders, Layers 2,4,6 are short ladders B.) Difference between short and long ladders is a total of 1.2in. C.) We are at the Westend looking east

Long ladders (from inside out, clockwise): L02B1, L04B1, L06B1, L08B1 L02B2, L04B2, L06B2, L08B2, L10B2, L12B2 L02B3, L04B3, L06B3, L08B3, L10B3, L12B2, L14B3, L16B3

Short ladders (from inside out, clockwise): L01B1, L03B1, L05B1, L07B1 L01B2, L03B2, L05B2, L07B2, L09B2, L11B2 L01B3, L03B3, L05B3, L07B3, L09B3, L11B3, L13B3, L15B3

Electronics Carrier definitions (Barrel 3):

Ladder A: wafers 1,2,3 - 4,5,6,7 (wafer labeling from E to W) Ladder B: wafers 1,2,3,4 - 5,6,7 (wafer labeling from E to W)

Ladder A:

Electronics Carriers labeling: 7NA (left looking from West) 7SA (right...)

7NA consists of 73L and 74R flat cables (order from East) 7SA consists of 73R and 74L flat cables (”)

Ladder B:

Electronics Carriers labeling: 7NB (left looking from West) 7SB (right...)

7NB consists of 74L and 73R flat cables (order from East) 7SB consists of 74R and 73L flat cables (”)

Electronics Carrier definition (Barrel 2): Only one ladder type Electronics Carrier labeling: 6N (left looking from West) 6S (right ...)

6N consists of 63L AND 63R flat cables (order from East) 6S consists of 63R and 63L flat cables (order from East)

Electronics Carrier definition (Barrel 1): Only one ladder type Electronics Carrier labeling: 4N (left looking from West) 4S (right ...)

4N consists of 42L AND 42R flat cables (order from East) 4S consists of 42R and 42L flat cables (order from East)

Ladder Definitions for Barrel 1 (Layers 1 and 2):

Ladder Size EC left EC right L01B1 short 4N (42L,42R) 4S (42R,42L) L02B1 long 4N (42L,42R) 4S (42R,42L) L03B1 short 4N (42L,42R) 4S (42R,42L) L04B1 long 4N (42L,42R) 4S (42R,42L) L05B1 short 4N (42L,42R) 4S (42R,42L) L06B1 long 4N (42L,42R) 4S (42R,42L) L07B1 short 4N (42L,42R) 4S (42R,42L) L08B1 long 4N (42L,42R) 4S (42R,42L)

Table 1.

Reference holes for Barrel 1 (from East Side of EC (upper left corner). Mark locations for South EC are same numbers but negative.

Ladder Mark 1 Mark 2 Mark 3 Mark 4 L01, L03, L05, L07 North EC 3.345 10.092 10.770 17.517 0.113 0.113 0.116 0.113 L02, L04, L06, L08 North EC 3.945 10.692 11.370 18.117 0.113 0.113 0.116 0.113

Ladder Definitions for Barrel 2 (Layers 3 and 4):

Ladder Size EC left EC right L01B2 short 6N (63L,63R) 6S (63R,63L) L02B2 long 6N (63L,63R) 6S (63R,63L) L03B2 short 6N (63L,63R) 6S (63R,63L) L04B2 long 6N (63L,63R) 6S (63R,63L) L05B2 short 6N (63L,63R) 6S (63R,63L) L06B2 long 6N (63L,63R) 6S (63R,63L) L07B2 short 6N (63L,63R) 6S (63R,63L) L08B2 long 6N (63L,63R) 6S (63R,63L) L09B2 short 6N (63L,63R) 6S (63R,63L) L10B2 long 6N (63L,63R) 6S (63R,63L) L11B2 short 6N (63L,63R) 6S (63R,63L) L12B2 long 6N (63L,63R) 6S (63R,63L)

Table 2.

Reference holes for Barrel 2 (from East Side of EC (upper left corner). Mark locations for South EC are same numbers but negative.

Ladder Mark 1 Mark 2 Mark 3 Mark 4 L01, L03, L05, L07, L09, L11 North EC 3.345 10.092 10.770 17.517 0.113 0.113 0.116 0.113 L02, L04, L06, L08, L10, L12 North EC 3.945 10.692 11.370 18.117 0.113 0.113 0.116 0.113

Ladder Definitions for Barrel 3 (Layers 5 and 6):

Ladder Size Category EC left EC right L01B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L02B3 long ladder B 7NB (74L,73R) 7SB (74R,73L) L03B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L04B3 long ladder B 7NB (74L,73R) 7SB (74R,73L) L05B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L06B3 long ladder B 7NB (74L,73R) 7SB (74R,73L) L07B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L08B3 long ladder B 7NB (74L,73R) 7SB (74R,73L) L09B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L10B3 long ladder B 7NB (74L,73R) 7SB (74R,73L) L11B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L12B3 long ladder B 7NB (74L,73R) 7SB (74R,73L) L13B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L14B3 long ladder B 7NB (74L,73R) 7SB (74R,73L) L15B3 short ladder A 7NA (73L,74R) 7SA (73R,74L) L16B3 long ladder B 7NB (74L,73R) 7SB (74R,73L)

Table 3.

Reference holes for Barrel 3 (from East Side of EC (upper left corner).

Ladder Mark 1 Mark 2 Mark 3 Mark 4 L01, L03, L05, L07, L09, L11, L13, L15 North EC 2.103 8.852 9.523 18.756 0.113 0.113 0.111 0.113 South EC -2.103 -8.850 -9.526 - 18.757 0.113 0.116 0.113 0.113 L02, L04, L06, L08, L10, L12, L14, L16 North EC 2.703 11.934 12.610 19.357 0.113 0.113 0.116 0.113 South EC -2.704 -11.937 -12.608 -19.537 0.113 0.111 0.113 0.113