40 bit bus

1-event memory

Trigger/ Control

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

Ctrl. FIFO Buffer

VME connector (with or without cable)

2:1 MUX

G-link

Laser Di.

Trigger Bus Fiber to DAQ

FE E C . FE E C .

FE E C . FE E C .

Master Slave

(2-4 Ctrl./FIFO/Buffers)

±8 V, Gnd.

Slow Ctrls.

HDLC Link