Aμ Guard leakage current

10^{-1} 1

Aμ Bias leakage current

0

0.5

1

1.5

2

2.5