RHIC Strobe, Pulser trigger (via TCD)

ADC Data (240 x 8 bit) to DSMI or ADC + timing data to DSMI

Analog out (buffered) testpoint (240)

Gate out (buffered) testpoint (16)

CTB 0.1 LG

Pulser Event Flag (1 x 1 bit) to DSM

0.1.3 CDB electronics to DSMI / DSM

ADC Data (240 x 8 bit)

LG October 19, 1998

0.1.1 CTB Tray (120)

charged particle tracks

slow controls (via VME) analog signals (2 x BNC / tray)

LED pulser (2 x BNC / tray)

0.1.2 HV Mainframe Supply

HV (2 x SHV / tray)

Discriminator out (240) (via P2 connector)