SVT Flex Cable Labeling Scheme

Version Number: 1.0 Date: 24-Aug-99 Input: SVT Electronics Carrier Assembly Scheme - August 99 Definitions:

Each Flex cable has its unique length LV cable attached to it. Thus each flex cable has to be uniquely labeled.

Flex Cable Labeling and LV cable lengths for Barrel 1 (Layers 1 and 2):

Ladder Flex Cable Label LV cable length L01B1 L01B1-N-42L 11.5 in L01B1-N-42R 11.5 in L01B1-S-42R 11.5 in L01B1-S-42L 11.5 in L02B1 L02B1-N-42L 12.5 in L02B1-N-42R 12.5 in L02B1-S-42R 12.5 in L02B1-S-42L 12.5 in L03B1 L03B1-N-42L 12.5 in L03B1-N-42R 12.5 in L03B1-S-42R 12.5 in L03B1-S-42L 12.5 in L04B1 L04B1-N-42L 12.5 in L04B1-N-42R 12.5 in L04B1-S-42R 12.5 in L04B1-S-42L 12.5 in L05B1 L05B1-N-42L 11.5 in L05B1-N-42R 11.5 in L05B1-S-42R 11.5 in L05B1-S-42L 11.5 in L06B1 L06B1-N-42L 12.5 in L06B1-N-42R 12.5 in L06B1-S-42R 12.5 in L06B1-S-42L 12.5 in L07B1 L07B1-N-42L 12.5 in L07B1-N-42R 12.5 in L07B1-S-42R 12.5 in L07B1-S-42L 12.5 in L08B1 L08B1-N-42L 12.5 in L08B1-N-42R 12.5 in L08B1-S-42R 12.5 in L08B1-S-42L 12.5 in

Table 1.

Flex Cable Labeling and LV cable lengths for Barrel 2 (Layers 3 and 4):

Ladder Flex Cable Label LV cable length L01B2 L01B2-N-63L 12.0 in L01B2-N-63R 12.0 in L01B2-S-63R 12.0 in L01B2-S-63L 12.0 in L02B2 L02B2-N-63L 9.5 in L02B2-N-63R 9.5 in L02B2-S-63R 9.5 in L02B2-S-63L 9.5 in L03B2 L03B2-N-63L 9.5 in L03B2-N-63R 9.5 in L03B2-S-63R 9.5 in L03B2-S-63L 9.5 in L04B2 L04B2-N-63L 11.5 in L04B2-N-63R 11.5 in L04B2-S-63R 11.5 in L04B2-S-63L 11.5 in L05B2 L05B2-N-63L 10.5 in L05B2-N-63R 10.5 in L05B2-S-63R 10.5 in L05B2-S-63L 10.5 in L06B2 L06B2-N-63L 9.5 in L06B2-N-63R 9.5 in L06B2-S-63R 9.5 in L06B2-S-63L 9.5 in L07B2 L07B2-N-63L 11.5 in L07B2-N-63R 11.5 in L07B2-S-63R 11.5 in L07B2-S-63L 11.5 in L08B2 L08B2-N-63L 10.5 in L08B2-N-63R 10.5 in L08B2-S-63R 10.5 in L08B2-S-63L 10.5 in

Table 2.

Barrel 2 (Layers 3 and 4) (continued):

Ladder Flex Cable Label LV cable length L09B2 L09B2-N-63L 9.5 in L09B2-N-63R 9.5 in L09B2-S-63R 9.5 in L09B2-S-63L 9.5 in L10B2 L10B2-N-63L 11.5 in L10B2-N-63R 11.5 in L10B2-S-63R 11.5 in L10B2-S-63L 11.5 in L11B2 L11B2-N-63L 9.5 in L11B2-N-63R 9.5 in L11B2-S-63R 9.5 in L11B2-S-63L 9.5 in L12B2 L12B2-N-63L 11.5 in L12B2-N-63R 11.5 in L12B2-S-63R 11.5 in L12B2-S-63L 11.5 in

Table 3.

Flex Cable Labeling and LV cable lengths for Barrel 3 (Layers 5 and 6):

Ladder Flex Cable Label LV cable length L01B3 L01B3-N-73L 9.0 in L01B3-N-74R 9.0 in L01B3-S-73R 9.0 in L01B3-S-74L 9.0 in L02B3 L02B3-N-74L 9.0 in L02B3-N-73R 9.0 in L02B3-S-74R 9.0 in L02B3-S-73L 9.0 in L03B3 L03B3-N-73L 9.0 in L03B3-N-74R 9.0 in L03B3-S-73R 9.0 in L03B3-S-74L 9.0 in L04B3 L04B3-N-74L 11.5 in L04B3-N-73R 11.5 in L04B3-S-74R 11.5 in L04B3-S-73L 11.5 in L05B3 L05B3-N-73L 9.0 in L05B3-N-74R 9.0 in L05B3-S-73R 9.0 in L05B3-S-74L 9.0 in L06B3 L06B3-N-74L 10.5 in L06B3-N-73R 10.5 in L06B3-S-74R 10.5 in L06B3-S-73L 10.5 in L07B3 L07B3-N-73L 11.5 in L07B3-N-74R 11.5 in L07B3-S-73R 11.5 in L07B3-S-74L 11.5 in L08B3 L08B3-N-74L 10.5 in L08B3-N-73R 10.5 in L08B3-S-74R 10.5 in L08B3-S-73L 10.5 in

Table 4.

Barrel 3 (Layers 5 and 6) (continued):

Ladder Flex Cable Label LV cable length L09B3 L09B3-N-73L 9.0 in L09B3-N-74R 9.0 in L09B3-S-73R 9.0 in L09B3-S-74L 9.0 in L10B3 L10B3-N-74L 9.0 in L10B3-N-73R 9.0 in L10B3-S-74R 9.0 in L10B3-S-73L 9.0 in L11B3 L11B3-N-73L 9.0 in L11B3-N-74R 9.0 in L11B3-S-73R 9.0 in L11B3-S-74L 9.0 in L12B3 L12B3-N-74L 11.5 in L12B3-N-73R 11.5 in L12B3-S-74R 11.5 in L12B3-S-73L 11.5 in L13B3 L13B3-N-73L 9.0 in L13B3-N-74R 9.0 in L13B3-S-73R 9.0 in L13B3-S-74L 9.0 in L14B3 L14B3-N-74L 10.5 in L14B3-N-73R 10.5 in L14B3-S-74R 10.5 in L14B3-S-73L 10.5 in L15B3 L15B3-N-73L 11.5 in L15B3-N-74R 11.5 in L15B3-S-73R 11.5 in L15B3-S-74L 11.5 in L16B3 L16B3-N-74L 11.5 in L16B3-N-73R 11.5 in L16B3-S-74R 11.5 in L16B3-S-73L 11.5 in

Table 5.