SVT HV Cable Labeling Scheme

Version Number: 1.1

Date: 25-Aug-99

Input: SVT Flex Cable Labeling Scheme - August 99

Definitions:

Each Ladder has two transition cards attached to it, one to the East side and one to the West Side. All transition cars are located on the water manifolds. The HV cables running between transition card and HV interface board have unique lengths based on the distance between the water manifold and the ladder.

The lengths in the following tables are measured from the edge of the HV interface board on the ladder to the face of the connector that engages on the transition board.

Transition Card Labeling / HV cable lengths (Barrel 1, Layers 1/2):

Ladder Transition Card Label HV cable length L01B1 TRDW01 7.0 in TRDE01 7.0 in L02B1 TRDW02 8.0 in TRDE02 8.0 in L03B1 TRUW05 8.0 in TRUE05 8.0 in L04B1 TRDW07 8.0 in TRDE07 8.0 in L05B1 TRDW10 7.0 in TRDE10 7.0 in L06B1 TRDW11 8.0 in TRDE11 8.0 in L07B1 TRUW14 8.0 in TRUE14 8.0 in L08B1 TRDW16 8.0 in TRDE16 8.0 in

Table 1.

Transition Card Labeling / HV cable lengths (Barrel 2, Layers 3/4):

Ladder Transition Card Label HV cable length L01B2 TRUW04 7.5 in TRUE04 7.5 in L02B2 TRDW04 5.0 in TRDE04 5.0 in L03B2 TRDW05 5.0 in TRDE05 5.0 in L04B2 TRUW08 7.0 in TRUE08 7.0 in L05B2 TRUW09 6.0 in TRUE09 6.0 in L06B2 TRDW09 5.0 in TRDE09 5.0 in L07B2 TRDW13 7.0 in TRDE13 7.0 in L08B2 TRUW13 6.0 in TRUE13 6.0 in L09B2 TRDW14 5.0 in TRDE14 5.0 in L10B2 TRUW17 7.0 in TRUE17 7.0 in L11B2 TRDW18 5.0 in TRDE18 5.0 in L12B2 TRUW18 7.0 in TRUE18 7.0 in

Table 2.

Transition Card Labeling / HV cable lengths (Barrel 3, Layers 5/6):

Ladder Transition Card Label HV cable length L01B3 TRUW01 4.5 in TRUE01 4.5 in L02B3 TRUW02 4.5 in TRUE02 4.5 in L03B3 TRUW03 4.5 in TRUE03 4.5 in L04B3 TRDW03 7.0 in TRDE03 7.0 in L05B3 TRDW06 4.5 in TRDE06 4.5 in L06B3 TRUW06 6.0 in TRUE06 6.0 in L07B3 TRUW07 7.0 in TRUE07 7.0 in L08B3 TRDW08 6.0 in TRDE08 6.0 in L09B3 TRUW10 4.5 in TRUE10 4.5 in L10B3 TRUW11 4.5 in TRUE11 4.5 in L11B3 TRDW12 4.5 in TRDE12 4.5 in L12B3 TRUW12 7.0 in TRUE12 7.0 in L13B3 TRUW15 4.5 in TRUE15 4.5 in L14B3 TRDW15 6.0 in TRDE15 6.0 in L15B3 TRUW16 7.0 in TRUE16 7.0 in L16B3 TRDW17 7.0 in TRDE17 7.0 in

Table 3.