SVT Fiber Labeling

Version Number: 1.0

Date: 26-Aug-99

Fibers were strung before the STAR comissioning run in May 99. LBL (Bob Minor) provided four 8-fiber bundles. Each bundle contains eight fibers, six for connections to the RDO boxes and two spares). Some of the spares are being used for the SSD.

The bundles were labeled: SVT SE Fibers DA-4 SVT SW Fibers DA-4 SVT NE Fibers DA-4 SVT NW Fibers DA-4 The DA-4 stands for DAQ rack 4.

Each individual fiber is labeled: SE-1 - SE-8 SW-1 - SW-8 NE-1 - NE-8 NW-1 - NW-8

The following page shows the translation of fiber labels to readout box labels.

RDO Box label fiber label RDOW01 SW-1 RDOW02 SW-2 RDOW03 SW-3 RDOW04 SW-4 RDOW05 SW-5 RDOW06 SW-6 RDOW07 NW-1 RDOW08 NW-2 RDOW09 NW-3 RDOW10 NW-4 RDOW11 NW-5 RDOW12 NW-6 RDOE01 SE-1 RDOE02 SE-2 RDOE03 SE-3 RDOE04 SE-4 RDOE05 SE-5 RDOE06 SE-6 RDOE07 NE-1 RDOE08 NE-2 RDOE09 NE-3 RDOE10 NE-4 RDOE11 NE-5 RDOE12 NE-6

Table 1.

2